
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "USB4120-03-C_REVA" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -12.7 16.002 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "USB4120-03-C_REVA" (id 1) (at -12.7 -18.542 0.0)
      (effects (font (size 1.27 1.27)) (justify top left))
    )
    (property "Footprint" "USB4120-03-C_REVA:GCT_USB4120-03-C_REVA" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Global Connector Technology" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "6.5mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "None" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/USB4120-03-C/Global+Connector+Technology/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "A" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/USB4120-03-C/Global+Connector+Technology/view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "USB4120-03-C" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            USB 2.0 Connector Type C Vertical Receptacle, 6.50mm profile, 16 Pins, Surface mount, Top mount, low profile, low cost\n                        \n" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "Not in stock" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "GCT" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "USB4120-03-C_REVA_0_0"
      (rectangle (start -12.7 -17.78) (end 12.7 15.24)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at -17.78 -10.16 0) (length 5.08)
        (name "GND_A"
          (effects (font (size 1.016 1.016)))
        )
        (number "A1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -17.78 -10.16 0) (length 5.08)
        (name "GND_A"
          (effects (font (size 1.016 1.016)))
        )
        (number "A12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -17.78 12.7 0) (length 5.08)
        (name "VBUS_A"
          (effects (font (size 1.016 1.016)))
        )
        (number "A4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -17.78 12.7 0) (length 5.08)
        (name "VBUS_A"
          (effects (font (size 1.016 1.016)))
        )
        (number "A9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 2.54 0) (length 5.08)
        (name "D1+"
          (effects (font (size 1.016 1.016)))
        )
        (number "A6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 5.08 0) (length 5.08)
        (name "CC1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -2.54 0) (length 5.08)
        (name "SBU1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 0.0 0) (length 5.08)
        (name "D1-"
          (effects (font (size 1.016 1.016)))
        )
        (number "A7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -17.78 -15.24 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -17.78 -15.24 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -17.78 -15.24 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -17.78 -15.24 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND_B"
          (effects (font (size 1.016 1.016)))
        )
        (number "B1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND_B"
          (effects (font (size 1.016 1.016)))
        )
        (number "B12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 12.7 180.0) (length 5.08)
        (name "VBUS_B"
          (effects (font (size 1.016 1.016)))
        )
        (number "B4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 12.7 180.0) (length 5.08)
        (name "VBUS_B"
          (effects (font (size 1.016 1.016)))
        )
        (number "B9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 0.0 180.0) (length 5.08)
        (name "D2+"
          (effects (font (size 1.016 1.016)))
        )
        (number "B6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -2.54 180.0) (length 5.08)
        (name "CC2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 5.08 180.0) (length 5.08)
        (name "SBU2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 2.54 180.0) (length 5.08)
        (name "D2-"
          (effects (font (size 1.016 1.016)))
        )
        (number "B7"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)