(footprint "Moisture_cap"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "pcb capacitor to measure moisture")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "22892f61-db4c-4e4a-bef6-919d3a58b757")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Untitled"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7ed236a2-6698-4f97-a468-24bc41988328")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6167c20c-d956-4a54-b71f-38a58a622dd3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d1ddbd67-6e06-4839-a4f9-74d4004afad7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_bom)
	(fp_line
		(start -7.5 65)
		(end -7.5 5)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "e2e2ce3e-82e1-45da-be7e-77c6c6dff80b")
	)
	(fp_line
		(start 6.5 7)
		(end -7.5 7)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "79db7641-d5f7-41fe-aa52-5e047171fe0d")
	)
	(fp_line
		(start 6.5 9)
		(end -7.5 9)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "5e4c158f-10c8-48d7-997a-545e002a25ba")
	)
	(fp_line
		(start 6.5 11)
		(end -7.5 11)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "2c16b902-6548-4172-81d4-09cb5b0dd905")
	)
	(fp_line
		(start 6.5 13)
		(end -7.5 13)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "fcb3301f-760b-4468-90d1-6be080cc5615")
	)
	(fp_line
		(start 6.5 15)
		(end -7.5 15)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "1ca5614d-e1f5-46b9-bfea-32fad4e94912")
	)
	(fp_line
		(start 6.5 17)
		(end -7.5 17)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "7f079aa3-f580-4bfb-a5f4-9629e9047a70")
	)
	(fp_line
		(start 6.5 19)
		(end -7.5 19)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "77086bda-2aaa-42a8-96ec-5723309f5478")
	)
	(fp_line
		(start 6.5 21)
		(end -7.5 21)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "ef4fe97e-3e08-46b3-9488-89adf762261c")
	)
	(fp_line
		(start 6.5 23)
		(end -7.5 23)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "11db49e1-ee84-40fa-a6d5-87312e0bf48c")
	)
	(fp_line
		(start 6.5 25)
		(end -7.5 25)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "2264c316-1e83-4af1-a2e9-449d9660a0e3")
	)
	(fp_line
		(start 6.5 27)
		(end -7.5 27)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "70a2a34d-df01-4521-991c-b2e85339e20b")
	)
	(fp_line
		(start 6.5 29)
		(end -7.5 29)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "5f687dba-05fa-4bb6-b03c-dba6da052482")
	)
	(fp_line
		(start 6.5 31)
		(end -7.5 31)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "3991303b-2121-45e8-8de7-15e9e03ed401")
	)
	(fp_line
		(start 6.5 33)
		(end -7.5 33)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "6b424e66-7263-4392-9a46-1ce9e5091315")
	)
	(fp_line
		(start 6.5 35)
		(end -7.5 35)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "6c0c58aa-632c-4834-8251-428fe275136f")
	)
	(fp_line
		(start 6.5 37)
		(end -7.5 37)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "47d0a217-c42c-44d7-95d9-f1709b37fe9a")
	)
	(fp_line
		(start 6.5 39)
		(end -7.5 39)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "1d63d106-80f5-4e80-9e3c-bf8daa166a06")
	)
	(fp_line
		(start 6.5 41)
		(end -7.5 41)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "b45bd750-54ae-459f-9aa5-87e59aef07fe")
	)
	(fp_line
		(start 6.5 43)
		(end -7.5 43)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "7d530925-f537-411c-af47-db8916b7d735")
	)
	(fp_line
		(start 6.5 45)
		(end -7.5 45)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "2a8a1a05-1766-49b4-99ca-ad44e61b4fcb")
	)
	(fp_line
		(start 6.5 47)
		(end -7.5 47)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "18a45e2c-08fa-49ef-9e1e-3b37bff1be8a")
	)
	(fp_line
		(start 6.5 49)
		(end -7.5 49)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "de7fc8c8-f2a9-436d-919a-e1541a8ae06d")
	)
	(fp_line
		(start 6.5 51)
		(end -7.5 51)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "3c10af4a-c80c-4406-96e9-56b2410ac853")
	)
	(fp_line
		(start 6.5 53)
		(end -7.5 53)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "32bcef6b-e617-4b9d-a9c2-8a88ce434a89")
	)
	(fp_line
		(start 6.5 55)
		(end -7.5 55)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "59096f8a-96bf-482b-b1e9-e09c93e2b202")
	)
	(fp_line
		(start 6.5 57)
		(end -7.5 57)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "474d81e3-a5f6-49cf-b4db-d4dc02deb9d8")
	)
	(fp_line
		(start 6.5 59)
		(end -7.5 59)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "07ce5e7d-08fe-45a0-97ef-3380dec1a4db")
	)
	(fp_line
		(start 6.5 61)
		(end -7.5 61)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "900514f0-578a-4539-aa7f-f75c4aaa53c9")
	)
	(fp_line
		(start 6.5 63)
		(end -7.5 63)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "ea52f367-9fea-4232-a140-4b21f972ea6f")
	)
	(fp_line
		(start 6.5 65)
		(end -7.5 65)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "07d077f7-35d8-4c64-a3be-68a85fed2de7")
	)
	(fp_line
		(start 7.5 5)
		(end 7.5 66)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "5c3487c8-15b6-4fce-905c-ac5202a3caa8")
	)
	(fp_line
		(start 7.5 8)
		(end -6.5 8)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "c3ffdea1-7b2d-4bb9-ad2d-66af3d7ea109")
	)
	(fp_line
		(start 7.5 10)
		(end -6.5 10)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "fd2be409-4922-4f77-bd5d-6e7c7ae0c710")
	)
	(fp_line
		(start 7.5 12)
		(end -6.5 12)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "bbb2664d-a727-4710-befe-ae4d923e9a89")
	)
	(fp_line
		(start 7.5 14)
		(end -6.5 14)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "1bfb3d88-c558-435f-89e1-91530a52d2ee")
	)
	(fp_line
		(start 7.5 16)
		(end -6.5 16)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "bbe696b9-abb8-4a6f-bc01-e5cedbc614d7")
	)
	(fp_line
		(start 7.5 18)
		(end -6.5 18)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "e5fb8c5d-0b0e-450a-aefc-170b521f714d")
	)
	(fp_line
		(start 7.5 20)
		(end -6.5 20)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "b83982ac-2b29-44e4-8570-01d461aa512d")
	)
	(fp_line
		(start 7.5 22)
		(end -6.5 22)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "be270b67-ce25-42bf-a935-3ea8de4dd244")
	)
	(fp_line
		(start 7.5 24)
		(end -6.5 24)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "267f564a-9fe8-4c1d-916b-bc609511e7d6")
	)
	(fp_line
		(start 7.5 26)
		(end -6.5 26)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "f31c4747-fab7-4c30-9517-4d3e2be36734")
	)
	(fp_line
		(start 7.5 28)
		(end -6.5 28)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "a49d5c69-495e-4bad-bbb3-54b2fe662e94")
	)
	(fp_line
		(start 7.5 30)
		(end -6.5 30)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "beacb6a8-c77b-4a2e-9e67-1ee001edb911")
	)
	(fp_line
		(start 7.5 32)
		(end -6.5 32)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "58298a86-8935-4342-9ee5-ef75fd29607b")
	)
	(fp_line
		(start 7.5 34)
		(end -6.5 34)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "4acecaff-435e-4b5e-82e6-1f1a39ec7044")
	)
	(fp_line
		(start 7.5 36)
		(end -6.5 36)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "1abf4f65-a122-48ac-8065-b693e3c5bcf1")
	)
	(fp_line
		(start 7.5 38)
		(end -6.5 38)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "59bb31cc-18b4-4bb5-b597-98bfa39e7d24")
	)
	(fp_line
		(start 7.5 40)
		(end -6.5 40)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "309c430a-2d85-4281-b9f5-3262c22f27f9")
	)
	(fp_line
		(start 7.5 42)
		(end -6.5 42)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "a42c0ca4-ca4e-4847-ab4b-4007469cb76e")
	)
	(fp_line
		(start 7.5 44)
		(end -6.5 44)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "2ca73e84-18ed-443d-8466-599b0ca1a08d")
	)
	(fp_line
		(start 7.5 46)
		(end -6.5 46)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "af26bc62-e6af-41b4-a530-98766291d7fb")
	)
	(fp_line
		(start 7.5 48)
		(end -6.5 48)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "681b0f93-5ab2-4f42-a583-f1c04c0b3e5f")
	)
	(fp_line
		(start 7.5 50)
		(end -6.5 50)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "3deb148b-d617-45ef-8c0d-9814b8733ff5")
	)
	(fp_line
		(start 7.5 52)
		(end -6.5 52)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "1e216d46-4759-4e82-b8c8-15e670e0fd82")
	)
	(fp_line
		(start 7.5 54)
		(end -6.5 54)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "1433164e-7499-49da-8cf9-0435b769620a")
	)
	(fp_line
		(start 7.5 56)
		(end -6.5 56)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "0085f2e5-25db-4023-aac8-82b019368906")
	)
	(fp_line
		(start 7.5 58)
		(end -6.5 58)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "a3535201-c850-4cec-8add-9c557460bd85")
	)
	(fp_line
		(start 7.5 60)
		(end -6.5 60)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "292ce834-c4ea-42dc-83b5-dc5de073b47b")
	)
	(fp_line
		(start 7.5 62)
		(end -6.5 62)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "86aa57a2-24d3-4452-a954-9d591eb12279")
	)
	(fp_line
		(start 7.5 64)
		(end -6.5 64)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "73b9676a-f786-47a9-a933-d846fbaee9fa")
	)
	(fp_line
		(start 7.5 66)
		(end -6.5 66)
		(stroke
			(width 0.5)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "d1c9aa36-a2ea-4631-a8c9-7fb3c91ac9a6")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cbaf74be-a9d9-490b-b735-d250e0f967b6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd circle
		(at -7.5 5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "38744740-4ba3-4381-b521-55ceac27a859")
	)
	(pad "2" smd circle
		(at 7.5 5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "5e769d5e-454e-4b95-927b-0470da0f766a")
	)
	(embedded_fonts no)
)
